(footprint "R_0805"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
	(tags "resistor")
	(property "Reference" "REF**"
		(at 0 -1.65 0)
		(layer "F.SilkS")
		(hide yes)
		(uuid "d9b3e3c5-0e4e-4cf4-b587-d5811bb8dac9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "3.3kΩ"
		(at 0 1.65 0)
		(layer "F.Fab")
		(uuid "91f9a1a1-bb18-4d06-b9ba-891afbeadf98")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010045_UNI-ROYAL-Uniroyal-Elec-0805W8F3301T5E_C26010.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c3e0c2d7-d5a9-4894-b3d4-3585f74fcb86")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "-55°C~+155°C 125mW 150V 3.3kΩ Thick Film Resistor ±1% ±100ppm/°C 0805 Chip Resistor - Surface Mount ROHS"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8e424ca0-ebad-438f-b20e-71522172fda8")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C26010"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "87a06b04-f03c-4ba1-b7ce-634fbc1873aa")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Stock" "2352266"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "548fc7e4-718a-4fdc-b18f-3c1404cb0472")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Price" "0.005USD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "86ba2cbb-8263-4bab-8b71-f0c2fe1a2ac0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Process" "SMT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "de51b013-fece-490f-8d04-fcb97bd26c6e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Minimum Qty" "20"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e119d535-9249-480e-85ad-22b28bd5733a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Attrition Qty" "10"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "9e7db069-ffc2-4fac-bffd-81d9c271f805")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Class" "Basic Component"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "24933108-fd4d-4956-ab86-e212169b7dd9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Category" "Resistors,Chip Resistor - Surface Mount"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aac5be14-8c3c-43a9-96a2-f17b61a1ef17")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer" "UNI-ROYAL(Uniroyal Elec)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a18c1cae-27f0-4607-8975-5920e66cdebf")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part" "0805W8F3301T5E"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3cbc2886-f6b4-4e75-822a-36dc35269415")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Resistance" "3.3kΩ"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "71cec837-ebdc-49b6-9c56-20c3cfcb7bc2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Power(Watts)" "125mW"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7de87f02-dd01-41cb-bc1a-07c173d7f891")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Type" "Thick Film Resistors"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b89bb1dc-29b7-4e27-9e58-9ae69143192c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Overload Voltage (Max)" "150V"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d708b91b-ef45-40f9-8923-d8b21ed085b5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Operating Temperature Range" "-55°C~+155°C"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "dd886a5d-deec-4966-8966-114e6179b0b8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Tolerance" "±1%"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f23cc797-a3c7-4e2d-8618-a12369659794")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Temperature Coefficient" "±100ppm/°C"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "6a4a885b-e195-4beb-b444-81968cf98a10")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.038)
	(attr smd)
	(fp_line
		(start -1.68 -0.95)
		(end 1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "fbf59772-8f79-460a-91c7-3d71198ca688")
	)
	(fp_line
		(start -1.68 0.95)
		(end -1.68 -0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "07593fb0-8432-4c18-bfd8-b259b457dcd8")
	)
	(fp_line
		(start 1.68 -0.95)
		(end 1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "a097a7fa-2467-4c6f-839d-8aaa732009c4")
	)
	(fp_line
		(start 1.68 0.95)
		(end -1.68 0.95)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e5d39d61-b841-4040-a37c-701138f7c60c")
	)
	(fp_line
		(start -1 -0.62)
		(end 1 -0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "777fea61-201f-4383-9d6f-e32beedfe1c7")
	)
	(fp_line
		(start -1 0.62)
		(end -1 -0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a0783f03-64b2-46e7-a2bc-05c32e5fb335")
	)
	(fp_line
		(start 1 -0.62)
		(end 1 0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "1a438e99-a458-45de-8cd3-faf81fa29513")
	)
	(fp_line
		(start 1 0.62)
		(end -1 0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "c17ce7cb-8c77-4354-a221-14fa60cab990")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
		(uuid "1fdd1e41-8cb1-4ade-9523-6af180efbbb7")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.91 0)
		(size 1.02 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.243902)
		(uuid "ac7d42cb-9ddd-492c-8667-dc4fa83364c5")
	)
	(pad "2" smd roundrect
		(at 0.91 0)
		(size 1.02 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.243902)
		(uuid "326d567e-4da8-483d-88c5-391af583ee02")
	)
	(embedded_fonts no)
	(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB.3dshapes/R_0805.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
