(footprint "SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL footprint")
	(tags "SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL footprint C7881")
	(property "Reference" "REF**"
		(at 0 -4.71 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "77d84188-f2cb-48d7-a2cc-76a71f54e8df")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "TPS54331DR"
		(at 0 4.71 180)
		(layer "F.Fab")
		(uuid "bd820558-b72c-4777-aa8a-d3b315df6f7d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_1808272040_Texas-Instruments-TPS54331DR_C9865.pdf"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "eabe8ef8-b2ab-4905-99b4-dd49547d3c7b")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "-40°C~+150°C@(TJ) 1 110uA 3.5V~28V 3A 570kHz 800mV~25V Adjustable Buck Buck Built-in No SOIC-8 DC-DC Converters ROHS"
		(at 0 0 180)
		(layer "F.Fab")
		(hide yes)
		(uuid "90089c9a-cd8e-4dd3-b55e-460c12298680")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C9865"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "344f3719-8cf0-4576-8aef-420376216b47")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Stock" "75356"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "71add6a9-47ae-4f0b-8080-184633b86858")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Price" "0.357USD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "249ff901-ef32-4697-88b2-59fb9858bce2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Process" "SMT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c9bef214-c437-462c-a6cd-d482d635d40e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Minimum Qty" "1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1e010911-dfdc-49a1-a81a-3ba8a1cfdf1b")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Attrition Qty" "0"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "3da78700-f49b-4e1e-afdc-dce0cce5c930")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Class" "Preferred Component"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ae624f06-1379-4f72-9798-cfc011fb82a0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Category" "Power Management ICs,DC-DC Converters"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0a8f6ffc-1e64-4c79-b388-8d249ba2f240")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer" "Texas Instruments"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5f4c0cd3-ef99-4c95-943b-5b077ba84f03")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part" "TPS54331DR"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e8185c77-d40d-4dcf-9446-e6c60e1acce8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Number Of Outputs" "1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e29c4180-276a-49b6-b097-90891ed18bbd")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Output Current (Max)" "3A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79661d92-92bb-41b2-a066-7e73fe4c98e6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Output Voltage" "0.8V~25V"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0f83e6b5-1ea2-41e0-bb25-8623b585e608")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Topology" "Step-down"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2e7dc7bc-a0c0-47c6-b0c9-7206eaac9017")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Synchronous Rectification" "No"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "42eb9a08-6ccd-4eee-a3ad-63c783528b42")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Switching Frequency" "570kHz"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "135d9c3c-06e1-46e6-b48a-797cdd6f0d90")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Input Voltage" "3.5V~28V"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b1ce9215-e8ae-49d7-b91e-8c18c1e87b4f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Output Type" "Adjustable"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "92352e9e-7c8d-43a9-af0e-271122cd4be9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Operating Temperature" "-40°C~+150°C@(TJ)"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "566cad3a-13fe-45b9-95e1-d600571bc508")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Function" "Step-down type"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "aebee203-ba75-4597-9a71-48e9c93dd175")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Switch Tube (Built-In/External)" "Built-in"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "367fe93f-6d0b-410a-a955-a82ed70c4db9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Quiescent Current (Iq)" "1mA"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "06b69de6-ddfe-4920-bd89-f12090684a01")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Output Current" "3A"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1b0d2f77-21f4-4731-a2c4-26e2911ae9e1")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.5 -1.91)
		(end -2.41 -1.91)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "8271e11a-c379-4176-b1fc-a6c5302427f6")
	)
	(fp_line
		(start -2.5 1.91)
		(end -2.5 -1.91)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "36ea7fc9-c5ae-47e7-a02f-40e027f404ce")
	)
	(fp_line
		(start -2.5 1.91)
		(end -2.41 1.91)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "acd40845-9fa7-4783-921e-e7abcaaed16e")
	)
	(fp_line
		(start 2.5 -1.91)
		(end 2.41 -1.91)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "47ac2a2a-6e3a-4caa-a60a-f589cc560e57")
	)
	(fp_line
		(start 2.5 -1.91)
		(end 2.5 1.91)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "bff172cd-f0bb-44de-aa51-9be76bdc8012")
	)
	(fp_line
		(start 2.5 1.91)
		(end 2.41 1.91)
		(stroke
			(width 0.15)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "317d3ebc-09f8-4812-875d-ca468f1f351d")
	)
	(fp_circle
		(center -2.5 2.25)
		(end -2.47 2.25)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "4eaa40f6-0856-4d02-a86b-25bc988b3f1d")
	)
	(fp_line
		(start -2.5 -2)
		(end 2.5 -2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "0c7420c8-cf57-40d5-8cce-b7cabf6b6967")
	)
	(fp_line
		(start -2.5 2)
		(end -2.5 -2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "abc50493-cffa-4a29-b95f-a7292d3a585f")
	)
	(fp_line
		(start 2.5 -2)
		(end 2.5 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "5018fa4d-18f5-427e-9b74-03bb8a348534")
	)
	(fp_line
		(start 2.5 2)
		(end -2.5 2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "301de3e7-b14d-48bc-b841-6db06f045a51")
	)
	(fp_circle
		(center -1.91 3.4)
		(end -1.75 3.4)
		(stroke
			(width 0.3)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "9b4d1531-2221-4fe1-9491-590f69a2b04c")
	)
	(fp_text user "REF**"
		(at 0 6.71 180)
		(layer "F.Fab")
		(uuid "00e39caa-beb5-445c-b6e1-ac8b8d837f79")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd oval
		(at -1.91 2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "77a31ff0-0fd4-4128-b73b-5e84d33ac8cf")
	)
	(pad "2" smd oval
		(at -0.64 2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "dbcfacae-e345-42ff-bd12-151b12a71de2")
	)
	(pad "3" smd oval
		(at 0.64 2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "4e4753a5-7838-4858-aef9-9111366b6219")
	)
	(pad "4" smd oval
		(at 1.91 2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "49e8772f-cdda-4b0f-8068-15c82c106f37")
	)
	(pad "5" smd oval
		(at 1.91 -2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "16b8352a-de95-47dc-864c-fee4072e2872")
	)
	(pad "6" smd oval
		(at 0.64 -2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "406d3391-9917-4cb7-bb1e-0e3a1d4da654")
	)
	(pad "7" smd oval
		(at -0.64 -2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "2d2316fb-ba6d-493b-bc0a-47141195533e")
	)
	(pad "8" smd oval
		(at -1.91 -2.71)
		(size 0.57 1.95)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "6a878046-8640-4f9f-a776-3b8d901d67bc")
	)
	(embedded_fonts no)
	(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB.3dshapes/SOIC-8_L5.0-W4.0-P1.27-LS6.0-BL.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
