(footprint "C_0805"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
	(tags "capacitor")
	(property "Reference" "REF**"
		(at 0 -1.68 180)
		(layer "F.SilkS")
		(hide yes)
		(uuid "c39c12b1-bc56-4b8c-afc5-6e4af4355ca5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "22uF"
		(at 0 1.68 180)
		(layer "F.Fab")
		(uuid "e1b25723-b117-4490-8f56-a71e687fee4e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_Samsung-Electro-Mechanics-CL21A226MAQNNNE_C45783.pdf"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ccd42fbc-d2ed-44b0-831b-84e73d7cac08")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "22uF 25V X5R ±20% 0805 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "79cafdd7-e484-4895-8211-6135c8dbc5d9")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "LCSC" "C45783"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "0f94f552-1c0d-4eab-b40d-640b9d599381")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Stock" "3493716"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5f9a587c-acb8-4516-a076-c403e0fb7be0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Price" "0.033USD"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "58f08235-63e5-4e1f-9528-00778bd0ea6a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Process" "SMT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "e0d225a2-2265-44eb-bdd1-3d917ed48b5c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Minimum Qty" "20"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "76ff3b2f-f473-436a-8ffc-94c822ac9aa5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Attrition Qty" "8"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c7d1b05b-f0b0-41bd-b5fd-1b4bd23fcc9d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Class" "Basic Component"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "a6f62ddd-eb25-43ba-9e0f-da9b58d8ad53")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Category" "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1d85de3b-885f-4c35-bbd1-874d5c1b6e6f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Manufacturer" "Samsung Electro-Mechanics"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "2f6bd73a-1ec2-4025-9c3d-0b39283a317c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Part" "CL21A226MAQNNNE"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "08d02ec9-2aff-4617-b561-5aac8c23e322")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Voltage Rated" "25V"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "78412994-d38a-44a1-91ce-64c5ad9644f9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Tolerance" "±20%"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "4349aa1e-0c4e-4ce4-9a95-f12529d8c098")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Capacitance" "22uF"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "8db23883-d8f9-4f69-8040-da9928cbda9a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Temperature Coefficient" "X5R"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "af07cc2d-0091-4d60-ad2a-5234da4d63b2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(solder_mask_margin 0.038)
	(attr smd)
	(fp_line
		(start -1.7 -1)
		(end 1.7 -1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "6212d79c-f2fe-4940-be0d-14b2f28947c8")
	)
	(fp_line
		(start -1.7 1)
		(end -1.7 -1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "e5332e13-b16e-4e19-8d72-cb1a97010746")
	)
	(fp_line
		(start 1.7 -1)
		(end 1.7 1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "eb7181c3-acc7-4de6-b042-642abb22ebd0")
	)
	(fp_line
		(start 1.7 1)
		(end -1.7 1)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "99a075c7-3f4b-400b-bbcc-b549e4a11d4e")
	)
	(fp_line
		(start -1 -0.62)
		(end 1 -0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "2afc455f-49c0-4a0a-84f3-5fa748c250b0")
	)
	(fp_line
		(start -1 -0.62)
		(end 1 -0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "44bd5915-6405-486d-a3d4-5c5fdbe5edff")
	)
	(fp_line
		(start -1 0.62)
		(end -1 -0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8faea929-fa3c-4848-a315-a01d1607af44")
	)
	(fp_line
		(start -1 0.62)
		(end -1 -0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f3d22ab1-25b0-4a13-8974-a44417daab8c")
	)
	(fp_line
		(start 1 -0.62)
		(end 1 0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8c0944a9-c517-4fea-951d-4dd25715894a")
	)
	(fp_line
		(start 1 -0.62)
		(end 1 0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "d6632fd1-718f-4e84-b46b-ab95e828ce13")
	)
	(fp_line
		(start 1 0.62)
		(end -1 0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "3c88a696-dd44-4fb5-bcd4-a8153d6c9ea6")
	)
	(fp_line
		(start 1 0.62)
		(end -1 0.62)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "b943510c-5b38-4366-9884-823bfcf21dc8")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
		(uuid "89302dcb-d6db-4802-bd10-e1260f5448d3")
		(effects
			(font
				(size 0.5 0.5)
				(thickness 0.08)
			)
		)
	)
	(pad "1" smd roundrect
		(at -0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "5e09d01e-fb2f-4b6c-85c2-a938bac5fade")
	)
	(pad "2" smd roundrect
		(at 0.95 0)
		(size 1 1.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(uuid "cd16a38f-3de1-4d64-ae1e-b85a733b0666")
	)
	(embedded_fonts no)
	(model "${KICAD8_3RD_PARTY}/3dmodels/com_github_CDFER_JLCPCB-Kicad-Library/JLCPCB.3dshapes/C_0805.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
