(kicad_sch
	(version 20260306)
	(generator "eeschema")
	(generator_version "10.0")
	(uuid "846f1443-bf1c-4671-963a-d559ca515f45")
	(paper "A4")
	(lib_symbols
		(symbol "74xGxx:74AHCT1G125"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at -2.54 3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "74AHCT1G125"
				(at 0 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_keywords" "Single Gate Buff Tri-State LVC CMOS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_fp_filters" "SOT* SG-*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(symbol "74AHCT1G125_0_1"
				(polyline
					(pts
						(xy -7.62 6.35) (xy -7.62 -6.35) (xy 5.08 0) (xy -7.62 6.35)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type background)
					)
				)
			)
			(symbol "74AHCT1G125_1_1"
				(pin input inverted
					(at 0 10.16 270)
					(length 7.62)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin input line
					(at -15.24 0 0)
					(length 7.62)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at -5.08 -10.16 90)
					(length 5.08)
					(name "GND"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "3"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin tri_state line
					(at 12.7 0 180)
					(length 7.62)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "4"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin power_in line
					(at -5.08 10.16 270)
					(length 5.08)
					(name "VCC"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "5"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "PCM_JLCPCB-Capacitors:0603,100nF"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "C"
				(at 2.032 1.668 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "100nF"
				(at 2.032 -0.3782 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 0.8 0.8)
					)
					(justify left)
				)
			)
			(property "Footprint" "PCM_JLCPCB:C_0603"
				(at -1.778 0 90)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2211101700_YAGEO-CC0603KRX7R9BB104_C14663.pdf"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Description" "100nF 50V X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "LCSC" "C14663"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Stock" "39955997"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Price" "0.006USD"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Process" "SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Minimum Qty" "20"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Attrition Qty" "10"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Class" "Basic Component"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Category" "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Manufacturer" "YAGEO"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Part" "CC0603KRX7R9BB104"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Voltage Rated" "50V"
				(at 2.032 -2.0462 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 0.8 0.8)
					)
					(justify left)
				)
			)
			(property "Tolerance" "±10%"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Capacitance" "100nF"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Temperature Coefficient" "X7R"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_fp_filters" "C_*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(symbol "0603,100nF_0_1"
				(polyline
					(pts
						(xy -1.27 0.635) (xy 1.27 0.635)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.27 -0.635) (xy 1.27 -0.635)
					)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "0603,100nF_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 3.175)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 3.175)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "PCM_JLCPCB-Resistors:0603,33Ω"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "R"
				(at 1.778 0 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 1.27 1.27)
					)
					(justify left)
				)
			)
			(property "Value" "33Ω"
				(at 0 0 90)
				(show_name no)
				(do_not_autoplace yes)
				(effects
					(font
						(size 0.8 0.8)
					)
				)
			)
			(property "Footprint" "PCM_JLCPCB:R_0603"
				(at -1.778 0 90)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010116_UNI-ROYAL-Uniroyal-Elec-0603WAF330JT5E_C23140.pdf"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Description" "-55°C~+155°C 100mW 33Ω 75V Thick Film Resistor ±1% ±100ppm/°C 0603 Chip Resistor - Surface Mount ROHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "LCSC" "C23140"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Stock" "2446304"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Price" "0.005USD"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Process" "SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Minimum Qty" "20"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Attrition Qty" "10"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Class" "Basic Component"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Category" "Resistors,Chip Resistor - Surface Mount"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Manufacturer" "UNI-ROYAL(Uniroyal Elec)"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Part" "0603WAF330JT5E"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Resistance" "33Ω"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Power(Watts)" "100mW"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Type" "Thick Film Resistors"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Overload Voltage (Max)" "75V"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Operating Temperature Range" "-55°C~+155°C"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Tolerance" "±1%"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Temperature Coefficient" "±100ppm/°C"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(symbol "0603,33Ω_0_1"
				(rectangle
					(start -1.016 2.54)
					(end 1.016 -2.54)
					(stroke
						(width 0.254)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "0603,33Ω_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "2"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "Symbols:GND"
			(power global)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+5V"
			(power global)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
				(show_name no)
				(do_not_autoplace no)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Footprint" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Datasheet" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(stroke
						(width 0)
						(type default)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name ""
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
					(number "1"
						(effects
							(font
								(size 1.27 1.27)
							)
						)
					)
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 123.19 86.36)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "0396d067-513d-4729-8091-b8c5da44cf36")
	)
	(junction
		(at 124.46 49.53)
		(diameter 0)
		(color 0 0 0 0)
		(uuid "4d022f2b-f314-4585-bb2d-7ecb3407ece1")
	)
	(hierarchical_label "IN_CMOS2"
		(shape input)
		(at 113.03 96.52 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right)
		)
		(uuid "adc3e357-d2db-4f79-ab92-740e05799062")
	)
	(hierarchical_label "OUT_5V_2"
		(shape input)
		(at 148.59 96.52 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left)
		)
		(uuid "c57e43d9-16b4-40b4-b231-65b200631f54")
	)
	(hierarchical_label "OUT_5V_1"
		(shape input)
		(at 149.86 59.69 0)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify left)
		)
		(uuid "ccabd83f-e7e7-44a8-8243-419351d9e2ce")
	)
	(hierarchical_label "IN_CMOS1"
		(shape input)
		(at 114.3 59.69 180)
		(effects
			(font
				(size 1.27 1.27)
			)
			(justify right)
		)
		(uuid "ce0e4f69-02a3-4d6f-8af7-1ab7b606961c")
	)
	(symbol
		(lib_id "PCM_JLCPCB-Resistors:0603,33Ω")
		(at 144.78 96.52 90)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "11666737-60c7-46a2-b1db-7e1f01dc9c88")
		(property "Reference" "R9"
			(at 144.78 92.71 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "33Ω"
			(at 144.78 96.52 90)
			(show_name no)
			(do_not_autoplace yes)
			(effects
				(font
					(size 0.8 0.8)
				)
			)
		)
		(property "Footprint" "PCM_JLCPCB:R_0603"
			(at 144.78 98.298 90)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010116_UNI-ROYAL-Uniroyal-Elec-0603WAF330JT5E_C23140.pdf"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "-55°C~+155°C 100mW 33Ω 75V Thick Film Resistor ±1% ±100ppm/°C 0603 Chip Resistor - Surface Mount ROHS"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "LCSC" "C23140"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Stock" "2446304"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Price" "0.005USD"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Process" "SMT"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Minimum Qty" "20"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Attrition Qty" "10"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Class" "Basic Component"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Category" "Resistors,Chip Resistor - Surface Mount"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Manufacturer" "UNI-ROYAL(Uniroyal Elec)"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Part" "0603WAF330JT5E"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Resistance" "33Ω"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power(Watts)" "100mW"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Type" "Thick Film Resistors"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Overload Voltage (Max)" "75V"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Operating Temperature Range" "-55°C~+155°C"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Tolerance" "±1%"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Temperature Coefficient" "±100ppm/°C"
			(at 144.78 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "48ea9720-d5f1-4f8c-a84b-1e5ee08b0dd9")
		)
		(pin "2"
			(uuid "0a91721b-a14e-45d5-9e05-bdfed290192c")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "R9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Symbols:GND")
		(at 115.57 86.36 180)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "14d35941-e897-4db5-84b0-4ddc3035954c")
		(property "Reference" "#PWR033"
			(at 115.57 80.01 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "GND"
			(at 115.57 81.28 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 115.57 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 115.57 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 115.57 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "3f1b058f-ec48-4224-a25c-c2dda47fa4e4")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR033")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_JLCPCB-Resistors:0603,33Ω")
		(at 146.05 59.69 90)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "3ec00810-2e29-4074-b3c7-b3351d8a8706")
		(property "Reference" "R3"
			(at 146.05 55.88 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "33Ω"
			(at 146.05 59.69 90)
			(show_name no)
			(do_not_autoplace yes)
			(effects
				(font
					(size 0.8 0.8)
				)
			)
		)
		(property "Footprint" "PCM_JLCPCB:R_0603"
			(at 146.05 61.468 90)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2206010116_UNI-ROYAL-Uniroyal-Elec-0603WAF330JT5E_C23140.pdf"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "-55°C~+155°C 100mW 33Ω 75V Thick Film Resistor ±1% ±100ppm/°C 0603 Chip Resistor - Surface Mount ROHS"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "LCSC" "C23140"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Stock" "2446304"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Price" "0.005USD"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Process" "SMT"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Minimum Qty" "20"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Attrition Qty" "10"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Class" "Basic Component"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Category" "Resistors,Chip Resistor - Surface Mount"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Manufacturer" "UNI-ROYAL(Uniroyal Elec)"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Part" "0603WAF330JT5E"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Resistance" "33Ω"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Power(Watts)" "100mW"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Type" "Thick Film Resistors"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Overload Voltage (Max)" "75V"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Operating Temperature Range" "-55°C~+155°C"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Tolerance" "±1%"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Temperature Coefficient" "±100ppm/°C"
			(at 146.05 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "56687ea2-6eff-47ff-92de-b2e0fe66287e")
		)
		(pin "2"
			(uuid "807b071d-6d62-4615-bcd9-bcb7adae0c18")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Symbols:GND")
		(at 128.27 86.36 180)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "44c96f15-769f-4eae-b63f-d981076c30a4")
		(property "Reference" "#PWR028"
			(at 128.27 80.01 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "GND"
			(at 128.27 81.28 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 128.27 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 128.27 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 128.27 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "74226a5a-e53c-4077-841b-b16d18f149e3")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR028")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 124.46 49.53 0)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "4a898f83-d3ee-4e65-8a3d-92e1a29040a1")
		(property "Reference" "#PWR023"
			(at 124.46 53.34 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "+5V"
			(at 124.46 44.45 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 124.46 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 124.46 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 124.46 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "783e0b76-0fa7-4eed-9445-f4fe404cf731")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR023")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_JLCPCB-Capacitors:0603,100nF")
		(at 120.65 49.53 270)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "586f9221-cae9-4e08-9fee-4fe8545e9e22")
		(property "Reference" "C8"
			(at 120.65 40.64 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "100nF"
			(at 120.65 43.18 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 0.8 0.8)
				)
			)
		)
		(property "Footprint" "PCM_JLCPCB:C_0603"
			(at 120.65 47.752 90)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2211101700_YAGEO-CC0603KRX7R9BB104_C14663.pdf"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "100nF 50V X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "LCSC" "C14663"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Stock" "39955997"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Price" "0.006USD"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Process" "SMT"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Minimum Qty" "20"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Attrition Qty" "10"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Class" "Basic Component"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Category" "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Manufacturer" "YAGEO"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Part" "CC0603KRX7R9BB104"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Voltage Rated" "50V"
			(at 120.65 45.72 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 0.8 0.8)
				)
			)
		)
		(property "Tolerance" "±10%"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Capacitance" "100nF"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Temperature Coefficient" "X7R"
			(at 120.65 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "039b20d2-82de-4da5-8404-fe331da43ca3")
		)
		(pin "2"
			(uuid "16c5fe9c-d466-4e9b-8c2b-04eada3da42a")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "C8")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Symbols:GND")
		(at 123.19 106.68 0)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "641860cb-3192-46db-b732-e37a2fef59cd")
		(property "Reference" "#PWR027"
			(at 123.19 113.03 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "GND"
			(at 123.19 111.76 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 123.19 106.68 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 123.19 106.68 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 123.19 106.68 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "2e1bb920-2754-4a39-a6dc-fb13e80d8fef")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR027")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Symbols:GND")
		(at 124.46 69.85 0)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "6916081b-a4c6-4daa-828c-107c17759249")
		(property "Reference" "#PWR024"
			(at 124.46 76.2 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "GND"
			(at 124.46 74.93 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 124.46 69.85 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 124.46 69.85 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 124.46 69.85 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "916bd5e2-8d57-436a-8334-8750395582c7")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR024")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 123.19 86.36 0)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "7a45c146-05ab-4da8-a8b5-1dedd1c4a663")
		(property "Reference" "#PWR026"
			(at 123.19 90.17 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "+5V"
			(at 123.19 81.28 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 123.19 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 123.19 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 123.19 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "f522e25d-3905-4844-93b8-c807fb74f267")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR026")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Symbols:GND")
		(at 116.84 49.53 180)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "c9cee43a-f1a8-426a-a9a1-04244ebdbb94")
		(property "Reference" "#PWR032"
			(at 116.84 43.18 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "GND"
			(at 116.84 44.45 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 116.84 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 116.84 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 116.84 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "615f1bd2-6ea9-48ed-a513-96237a1d3785")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR032")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xGxx:74AHCT1G125")
		(at 129.54 59.69 0)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "da05db13-a6d1-48f7-8c53-17a69da17206")
		(property "Reference" "U2"
			(at 142.24 53.2698 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74AHCT1G125"
			(at 142.24 55.8098 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "PCM_JLCPCB:SOT-23-5_L3.0-W1.7-P0.95-LS2.8-BL"
			(at 129.54 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 129.54 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 129.54 59.69 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "4"
			(uuid "bcfadd9e-048e-4add-a1b8-c49cbb77fca6")
		)
		(pin "1"
			(uuid "766e7f0c-5123-40d9-acec-aeb1e973cc2d")
		)
		(pin "2"
			(uuid "befc87c8-708a-4296-9fa5-3576847f8c6f")
		)
		(pin "5"
			(uuid "01d513a7-7289-4139-ad1a-be0a4c203757")
		)
		(pin "3"
			(uuid "7dd7bbc5-cbb2-4e36-a106-ae198e3020bc")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "U2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_JLCPCB-Capacitors:0603,100nF")
		(at 119.38 86.36 270)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "e8dab4c5-9cd5-4150-8775-599df147d7dc")
		(property "Reference" "C9"
			(at 119.38 77.47 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "100nF"
			(at 119.38 80.01 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 0.8 0.8)
				)
			)
		)
		(property "Footprint" "PCM_JLCPCB:C_0603"
			(at 119.38 84.582 90)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2211101700_YAGEO-CC0603KRX7R9BB104_C14663.pdf"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "100nF 50V X7R ±10% 0603 Multilayer Ceramic Capacitors MLCC - SMD/SMT ROHS"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "LCSC" "C14663"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Stock" "39955997"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Price" "0.006USD"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Process" "SMT"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Minimum Qty" "20"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Attrition Qty" "10"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Class" "Basic Component"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Category" "Capacitors,Multilayer Ceramic Capacitors MLCC - SMD/SMT"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Manufacturer" "YAGEO"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Part" "CC0603KRX7R9BB104"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Voltage Rated" "50V"
			(at 119.38 82.55 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 0.8 0.8)
				)
			)
		)
		(property "Tolerance" "±10%"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Capacitance" "100nF"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Temperature Coefficient" "X7R"
			(at 119.38 86.36 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "8ab6b16c-5be9-4b69-96f3-ab990c86e0d7")
		)
		(pin "2"
			(uuid "f443f533-747e-4e06-ab4f-e97bca696fdd")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "C9")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "74xGxx:74AHCT1G125")
		(at 128.27 96.52 0)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "eed6a8b2-6afa-4cab-9391-d4a85ca7fddb")
		(property "Reference" "U4"
			(at 140.97 90.0998 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "74AHCT1G125"
			(at 140.97 92.6398 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" "PCM_JLCPCB:SOT-23-5_L3.0-W1.7-P0.95-LS2.8-BL"
			(at 128.27 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf"
			(at 128.27 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Single Buffer Gate Tri-State, Low-Voltage CMOS"
			(at 128.27 96.52 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "4"
			(uuid "d9c900a5-a344-4954-a56c-9dc57ed5cee9")
		)
		(pin "1"
			(uuid "0eedcf7e-b762-4ca0-aa0b-f6cfcaee7ba1")
		)
		(pin "2"
			(uuid "a0e426f5-436b-4f35-8102-2164729d1cb2")
		)
		(pin "5"
			(uuid "7b4947d3-8b0c-47cb-8a70-9ce4f96ff922")
		)
		(pin "3"
			(uuid "25fe3cbd-e442-4fb7-b5f3-ac3f7f7fbab9")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "U4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Symbols:GND")
		(at 129.54 49.53 180)
		(unit 1)
		(body_style 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(dnp no)
		(fields_autoplaced yes)
		(uuid "f095c92a-1129-4189-af03-887fe062bf48")
		(property "Reference" "#PWR025"
			(at 129.54 43.18 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "GND"
			(at 129.54 44.45 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 129.54 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" ""
			(at 129.54 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 129.54 49.53 0)
			(hide yes)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(pin "1"
			(uuid "81d64865-1ebc-4e44-9594-ef85b82f3c12")
		)
		(instances
			(project "WLED_Controlboard"
				(path "/038eac60-c432-4a46-9e68-0e61aa44e7bf/f1d06a97-cc23-43e1-aab1-5a16b4a02c03"
					(reference "#PWR025")
					(unit 1)
				)
			)
		)
	)
)
