(footprint "WEMOS_D1_mini_light"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "16-pin module, column spacing 22.86 mm (900 mils), https://wiki.wemos.cc/products:d1:d1_mini, https://c1.staticflickr.com/1/734/31400410271_f278b087db_z.jpg")
	(tags "ESP8266 WiFi microcontroller")
	(property "Reference" "REF**"
		(at 22 27 180)
		(layer "F.SilkS")
		(uuid "ec258290-6703-476a-b6bd-627ccd129fd6")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "WEMOS_D1_mini"
		(at 11.7 0 180)
		(layer "F.Fab")
		(uuid "0ff764c6-c1d1-429f-b435-11cc9094c25d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" "https://wiki.wemos.cc/products:d1:d1_mini#documentation"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "5cebfe2f-c94a-4e1c-ab86-ee9fd1c714e7")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "32-bit microcontroller module with WiFi"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "c55fcf14-62b9-4b34-8e6b-363b9350fb7c")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -1.5 19.22)
		(end -1.5 -6.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "ffe25c45-1745-4fc2-a116-85d89e291d12")
	)
	(fp_line
		(start -1.5 19.22)
		(end 1.04 19.22)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "2cfcf552-562d-44ff-a31b-85eef8957549")
	)
	(fp_line
		(start 1.04 19.22)
		(end 1.04 26.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "cf4994a6-d01f-4555-ab16-3fda48090541")
	)
	(fp_line
		(start 1.04 26.12)
		(end 24.36 26.12)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "367c7b5e-ae98-4457-87b6-b78186239c8e")
	)
	(fp_line
		(start 22.24 -8.34)
		(end 0.63 -8.34)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "c5dc81b6-3abf-4b5a-b888-24973080766a")
	)
	(fp_line
		(start 24.36 26.12)
		(end 24.36 -6.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "e514444c-36da-42f1-9fe9-bd87065193c1")
	)
	(fp_arc
		(start -1.5 -6.21)
		(mid -0.876137 -7.716137)
		(end 0.63 -8.34)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "90939dc7-93d7-4d6f-ab92-06c09d94e7e7")
	)
	(fp_arc
		(start 22.23 -8.34)
		(mid 23.736137 -7.716137)
		(end 24.36 -6.21)
		(stroke
			(width 0.12)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "b0c66283-3d19-461b-be84-f0fea6ea0c3c")
	)
	(fp_poly
		(pts
			(xy -2.54 -0.635) (xy -2.54 0.635) (xy -1.905 0)
		)
		(stroke
			(width 0.15)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "11821841-2665-4313-961f-2667659b86eb")
	)
	(fp_line
		(start -1.62 -8.46)
		(end 24.48 -8.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "ca30d9a3-e366-4eb0-828f-887dbb236b92")
	)
	(fp_line
		(start -1.62 26.24)
		(end -1.62 -8.46)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "2bb464b8-18b9-42f1-b5ac-13eeb6cc7383")
	)
	(fp_line
		(start 24.48 -8.46)
		(end 24.48 26.24)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "594ef72f-260b-4f5c-9b75-94293d389df2")
	)
	(fp_line
		(start 24.48 26.24)
		(end -1.62 26.24)
		(stroke
			(width 0.05)
			(type solid)
		)
		(layer "F.CrtYd")
		(uuid "c2f1abf7-2572-4128-a3c1-928df8eba120")
	)
	(fp_line
		(start -1.37 -6.21)
		(end -1.37 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "9fb7b4af-bbe0-4c42-aee9-ca235beb18aa")
	)
	(fp_line
		(start -1.37 1)
		(end -1.37 19.09)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "579bbc95-40c1-492a-90f3-6541155c87ac")
	)
	(fp_line
		(start -1.37 1)
		(end -0.37 0)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "8a2cb3ca-3721-4d40-b2d2-0d27b0bd2e55")
	)
	(fp_line
		(start -1.37 19.09)
		(end 1.17 19.09)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "4d5ed9c9-6ac4-4255-a3cd-f9a7b9434c25")
	)
	(fp_line
		(start -0.37 0)
		(end -1.37 -1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "7d365bbb-c0b9-413d-8139-24f62984872b")
	)
	(fp_line
		(start 1.17 19.09)
		(end 1.17 25.99)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ea15cae4-89c3-4721-9d6a-ec50113b8104")
	)
	(fp_line
		(start 1.17 25.99)
		(end 24.23 25.99)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "ea504522-5e1a-4a1f-a32c-7fc0495b9f21")
	)
	(fp_line
		(start 22.23 -8.21)
		(end 0.63 -8.21)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "e4210c06-9a27-4a7e-a9a2-b70fe07f2ca9")
	)
	(fp_line
		(start 24.23 25.99)
		(end 24.23 -6.21)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "f3d573aa-31f9-4a67-b785-e1761b5a03a4")
	)
	(fp_arc
		(start -1.37 -6.21)
		(mid -0.784214 -7.624214)
		(end 0.63 -8.21)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "cce02169-7c55-49f2-8ca5-c41303b5b4c3")
	)
	(fp_arc
		(start 22.25 -8.21)
		(mid 23.658356 -7.610071)
		(end 24.23 -6.19)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "6f565926-7d67-4dd5-a814-737c594302b0")
	)
	(fp_text user "No copper"
		(at 11.43 -3.81 180)
		(layer "Cmts.User")
		(uuid "0da6b272-df6b-48b4-926d-61f16de1c19e")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(fp_text user "${REFERENCE}"
		(at 11.43 10 180)
		(layer "F.Fab")
		(uuid "5ecd174a-d06b-4b1b-9cf1-da87c93a300c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 2 2)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d61a5fc6-d8f9-4749-9f83-3868cee0f65f")
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "fdb03264-5f97-44a4-8f55-0bd0110da112")
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "a83a1620-3fca-4e00-8b8a-61c7b6c6c400")
	)
	(pad "4" thru_hole oval
		(at 0 7.62)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "640e7774-a29e-4383-97f1-d23b51de96b0")
	)
	(pad "5" thru_hole oval
		(at 0 10.16)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d57fdc2c-773c-4815-9300-2809cd6b24a1")
	)
	(pad "6" thru_hole oval
		(at 0 12.7)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "176a6f41-eb41-4cff-8d96-b4bd08cebde2")
	)
	(pad "7" thru_hole oval
		(at 0 15.24)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "33f47674-173e-4ba9-a080-d51387db24e3")
	)
	(pad "8" thru_hole oval
		(at 0 17.78)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "1638e7e8-d053-4f81-ab42-19fcd3cb9e42")
	)
	(pad "9" thru_hole oval
		(at 22.86 17.78)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "4539bff2-62d6-47d8-8569-255d43d0f4ae")
	)
	(pad "10" thru_hole oval
		(at 22.86 15.24)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "d04794a3-27b7-4790-b2a7-06dd43091693")
	)
	(pad "11" thru_hole oval
		(at 22.86 12.7)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "51643f96-5735-4cb5-a956-616b5528e7bd")
	)
	(pad "12" thru_hole oval
		(at 22.86 10.16)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "823d8b52-cb38-4127-92a1-f1b16c4afedc")
	)
	(pad "13" thru_hole oval
		(at 22.86 7.62)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e50d1d71-da22-48ba-924c-917d4bbc339d")
	)
	(pad "14" thru_hole oval
		(at 22.86 5.08)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6e3eca3a-f202-4c19-a2a3-9e9d6be71216")
	)
	(pad "15" thru_hole oval
		(at 22.86 2.54)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "5d2eec50-49da-42cf-a3c9-872490a8d83e")
	)
	(pad "16" thru_hole oval
		(at 22.86 0)
		(size 2 1.6)
		(drill 0.9)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "9bb92773-0322-417d-bf9f-8feb50677b3b")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "Dwgs.User")
		(uuid "1b8adb44-c957-4913-bf02-c890fb4565d8")
		(name "No Copper")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 56.420001 190.480001) (xy 82.020001 190.480001) (xy 82.020001 197.280001) (xy 56.420001 197.280001)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/WEMOS_D1_mini_light.step"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
